1.  unzip the firmware package 
2.  Connect the ILD2300  („Ethernet“ female connector) to a PC using an Ethernet direct connection (LAN). 
    Use a LAN cable with RJ-45 connectors.
3.  start UpdateSensor.exe which will automatically connect with the sensor
4.  choose the firmware file *.meu
5.  start update

